**SECTION 605 — UNDERDRAINS**

Make the following amendments to said Section:

**(I)** Amend **605.04 - Measurement** lines 60 to 61 to read as follows:

**"605.04 Measurement.**

1. The Engineer will measure underdrains per linear feet in accordance with the contract documents.

**(B)** The Engineer will measure underdrain outlet and cleanout per each in accordance with the contract documents."

**(II)** Amend 605.05 - Payment lines 63 to 76 to read as follows:

**"605.05 Payment.** The Engineer will pay for the accepted pay item listed below at contract price per pay unit, as shown in the proposal schedule. Payment will be full compensation for the work prescribed in this section and the contract documents.

 The Engineer will pay for the following pay item when included in the proposal schedule:

 **Pay Item Pay Unit**

 Inch Underdrain Linear Foot

**(1)** 40% of the contract unit price upon completion of excavating to the required dimensions and grade.

**(2)** 20% of the contract unit price upon completion of installing geotextile fabric.

**(3)** 40% of the contract unit price upon completion of placing untreated permeable base and perforated pipe and wrapping geotextile fabric.

Type Underdrain Outlet Each

Cleanout Each"

**END OF SECTION 605**