**SECTION 611 — HAND-LAID RIPRAP**

Make the following amendments to said Section:

1. Amend **611.02 - Materials** line 8 to read as follows:

"Geotextiles for Stabilization Applications 716.06"

**(II)** Amend **611.04 - Measurement** lines 28 to 29 to read as follows:

**"611.04 Measurement.** The Engineer will measure hand-laid riprap per cubic yard in accordance with the contract documents."

**(III)** Amend **611.05 - Payment** lines 31 to 43 to read as follows:

**"611.05 Payment.** The Engineer will pay for the accepted pay item listed below at contract price per pay unit, as shown in the proposal schedule.

Payment will be full compensation for the work prescribed in this section and the contract documents.

The Engineer will pay for the following pay item when included in the proposal schedule:

**Pay Item Pay Unit**

Hand-Laid Riprap Cubic Yard

1. 40% of the contract unit price upon completion of excavating to the required depth and preparing the foundation bed.

**(2)** 20% of the contract unit price upon completion of installing geotextile fabric.

**(3)** 40% of the contract unit price upon completion of placing and distributing stones and removing and replacing displaced or damaged geotextile fabric damaged during riprap placement."

**END OF SECTION 611**