**SECTION 207 — DITCH AND CHANNEL EXCAVATION**

Make the following amendments to said Section:

**(I)** Amend **207.04 - Measurement** by revising lines 35 to 41 to read as follows:

 **"207.04 Measurement.**

The Engineer will measure ditch and channel excavation per cubic yard in accordance with the contract documents. Excavation will be measured after clearing and grubbing."

**(II) Amend 207.05 - Payment** by revising lines 43 to 961 to read as follows:

**"207.05 Payment.** The Engineer will pay for the accepted pay item listed below at the contract price per pay unit, as shown in the proposal schedule. Payment will be full compensation for the work prescribed in this section and the contract documents.

 The Engineer will pay for the following pay item when included in the proposal schedule:

 **Pay Item Pay Unit**

Ditch and Channel Excavation Cubic Yard

**(1)** 80% of the contract bid price upon completion of clearing and grubbing, excavating ditch, and backfilling and compacting below required bottom grade of ditches and channels.

**(2)** 20% of the contract bid price upon completion of disposing unsuitable and surplus material.

 The Engineer will not pay for clearing and grubbing in accordance with Section 201- Clearing and Grubbing.

**END OF SECTION 207**